EXPRESSION OF INTEREST (EOI)

**EOI Reference #: AKSO-STJ-2023-006**

**BIDS Categories: 2800, 9400,9800, 5800**

**Aker Solutions Website:** [http://www.akersolutions.com/Can-procurement](https://eur01.safelinks.protection.outlook.com/?url=http%3A%2F%2Fwww.akersolutions.com%2FCan-procurement&data=05%7C01%7CGeorge.Parsons%40akersolutions.com%7C9fee4df02375465dcec508db89d2f014%7C26b749f68c7244e3bbdeae3de07b4206%7C0%7C0%7C638255311283957789%7CUnknown%7CTWFpbGZsb3d8eyJWIjoiMC4wLjAwMDAiLCJQIjoiV2luMzIiLCJBTiI6Ik1haWwiLCJXVCI6Mn0%3D%7C3000%7C%7C%7C&sdata=ssV7GHEzC3rK24g4b%2Bj5bwGrQPkouWJzyrmZoVMHZyU%3D&reserved=0)

**Title: Welding Execution, Fabrication and Craft Labour**

**Project: Cenovus - West White Rose Project (WWRP)**

**Issue Date: July 25, 2023**

**Closing Date: August 15, 2023**

**GENERAL**

Aker Solutions hereby invites interested parties to submit an Expression of Interest (EOI) in relation to the scope of work associated with the hook-up and commissioning services for the Cenovus West White Rose Project in Newfoundland and Labrador, Canada. Aker Solutions is pre-qualifying suppliers interested in providing services specified below that will be executed by industry standards and best-value work practices.

**DIVERSITY**

Aker Solutions encourages the participation of members of designated groups, and corporations or cooperatives owned by them, in the supply of goods and services.

**SCOPE OF SERVICES**

**Onshore Preparation & Offshore Execution of Hook-up Welding Scopes**

To develop all structural and piping weld procedures and ITPs required for the WWRP Hook-up offshore Newfoundland and Labrador, including the provision of qualified welding personnel to execute the scope of work.

**Pipe material weld requirements:**

* 24"SCH 40 A-333 GR 6 SMLS,
* 20" SMLS 15.09mm WT BE CS API 5L X52,
* 12” Sch 40A-358 GR 316/316L CL1,
* 16” Sch 40 B-862 GR 2,
* 12” Sch 120 A-790 UNS S32750 SMLS,
* 10" Sch 160 A-790 UNS S32750 SMLS,
* 8” 39.0mm WT A-333 GR 6 SMLS and
* 32” 25.4mm WT BE CS API 5L X52.

**Structural welding requirements:**

Welding Process - SMAW/FCAW Thickness base material ranges 6mm - 250mm (Including Fracture Mechanics (CTOT)) Material Grade S355 – S460 – CJP, PJP and FW Minimum groove angle 30 deg or more.

**Onshore Preparations for Offshore Execution:**

Execute onshore mock-ups to further define the offshore scope and ensure execution certainty.

Partial assembly of submersible pump strings, firewater, and seawater.

Provision of fabrication facility for structural welder training and qualifications in early 2024.

Provision of a fabrication facility for structural and pipe welder training and qualifications in late 2024 in preparation for offshore execution.

**Offshore Execution Scope**

Supply of qualified personnel and Welding Equipment to execute the hook-up of the WWRP offshore are estimated as follows:

**Estimated personnel requirements based on the current plan are:**

Eighty (80) Structural Welders (all qualified to weld module leg connection)

Thirty (30) Ironworkers

Thirty (30) Pipe Welders (Super Duplex, Stainless, titanium, LTCS ETC.)

Twenty (20) Pipe Fitters

Thirty (30) Mechanical Technicians

Thirty (30) Electrical Technicians

Twelve (12) Instrument Technicians

All tooling and equipment necessary for weld qualification and training is the contractor’s responsibility.

All offshore trades shall be red seal certified journeypersons.

Industry and Regulatory training for working offshore NL is the contractor’s responsibility.

**TENTATIVE SCHEDULE**

Offshore welding scope - Q3 2025

Topsides installation – July 2025

Hook-up execution to follow immediately after topside installation.

**SUBMISSION REQUIREMENTS**

As part of the submission requirements, suppliers are requested to provide Aker Solutions with the following answers and/or information:

1. Are you pre-qualified under the Aker Solutions Ariba System? **YES/NO.**

If “**YES”**, then please provide.

* Ariba SAP number.

If “**NO**”, then please provide the following:

* A brief outline of the following company information:
  1. Copy of Certificate of Incorporation.
  2. Company Name and Address.
  3. Single Point of Contact, c/w contact details.
  4. Organizational Chart.

1. Completeand respond to all questions in the attached Pre-Qualification questionnaire**.**

**Note:**

Only those respondent(s) who are successful in pre-qualifying will be invited to submit priced commercial proposals at the bid stage.

**RESPONSE REQUIREMENTS**

Suppliers are to respond to the following e-mail address:

[**Subcontracts.STJ.Department@akersolutions.com**](mailto:Subcontracts.STJ.Department@akersolutions.com)

on or before the closing date noted above.

The subject line of the email must contain the following:

**EOI REFERENCE NUMBER – TITLE – Supplier Company Name**

Suppliers that have not been pre-qualified previously in Ariba will be required to do so before Aker Solutions will issue any formal RFQ/Tender/Bid packages.

If you have any questions regarding this announcement, please contact Aker Solutions Single Point of Contact listed below:

Renee Payne

Contract Administrator

Aker Solutions Canada Inc.

[Renee.Payne@akersolutions.com](mailto:Renee.Payne@akersolutions.com)